**The 5-4-3-2-1 Rule in Networking**

Maimoona Khilji

Institute of Management Science

Course Code: Data Communication and Computer Networking

Zahid ullah

18th October, 2021

The 5-4-3-2-1 Rule

in Networking

The 5-4-3-2-1 rule is basically a design specification for a network. It represents the creation of single collision domain. A **single collision domain** is a segment of cable over which two stations can’t communicate the data at the same time. If the communication occurs, collision will happen. According to the rule, in one network, only five segments can be created having four repeaters, three populated segments and two link segments.

The 5-4-3-2-1 rule can explained as:

5 - The number of Segments






4 - The number of repeaters

3 - The number of Populated Segments



2 - The number of link segments (or unpopulated segments)

1 - The number of Network

**Link Segment**



**Repeater**



**Repeater**

**Repeater**

**Repeater**

**Populated Segments**

**Populated Segments**

**Populated Segments**

**Link Segment**

Figure Representation of 5-4-3-2-1 Rule

**IMPORTANT TERMS:**

**Segment:** A portion of a computer network that is separated from the rest of the

network by devices such as a hub, repeater is known as segment.

**Repeater:** An electronic device that regenerates or boost up the weak signals so

that it can go further is known as repeater.

**Populated segments:** Segments that are connected to terminals of repeater are

known as populated segments.

**Link segments:** Segments that are not connected to terminals of repeater are

known as link segments.

**Network:** A data communication system in which two or more entities are

connected to each other through some transmission medium in order

to share **data** and **resources.**